**How to Use the AEG Ceramic Hob**

**Other than suitable cookware please do not put other items on the ceramic surface**

**Activating the hob**

* Hob shut off switch is in the cupboard right-hand side – currently quite stiff be firm but not rough
* Pushing the lever **UP** the Hob will be operational
* **On the hob itself, Use the ON / OFF sensor on the immediate left to activate or deactivate the hob**

**Heat Setting**

* Use the control bar (centre front) To set or change the heat setting
* Touch the control bar at the correct heat setting or move your finger along the control bar until you reach the correct heat setting

**Activating and deactivating the outer rings**

* You can adjust the surface you cook, to the dimension of the cookware, using the sensor relevant to the field to expand zone or decrease zone

**Deactivating the hob**

* **On the hob itself, Use the ON / OFF sensor on the immediate left to activate or deactivate the hob**
* Hob shut off switch is in the cupboard right-hand side – currently quite stiff be firm but not rough
* Pushing the lever **DOWN** the Hob will cease to be operational

**Cleaning the ceramic hob**

* Do not use any abrasive cleaning implement ie scourer , wire wool
* The preferred hob cleaner can be found in the top cupboard nearest the door
* Squeeze a small amount on the **COOL** ceramic surface, wipe over surface gently removing any stubborn spills. Rinse cloth, wipe surface again and dry off with tea towel

**Chinnor Village Hall Committee ask all Users of the kitchen equipment to leave it in a clean and useable condition ready for others**