**How to Use the Haier Wine Cooler**

**Switching on and acclimatisation**

* Wine cooler power switch located on the wall
* Wait 30 minutes to acclimatise before making any temperature adjustments
* The default settings are 12°C

The Wine Cooler can be set to any temperature you wish so as to accommodate your wine storage requirements.

* To set the temperature hold the button for approx. 3 seconds
* The temperature display will blink
* Press the + or – buttons to increase or decrease the temperature setting
* Once desired temperature is attained press the button or stop operation (approx. 5 seconds)
* The panel will memorise the setting

The temperature display will revert back to display the inside temperature

It may take some time to reach the set temperature

To change from C° to F° press the  button about 3 seconds

**Turn the Wine Cooler OFF on completion of your event**